Driver package for CUSTOM VKP80III printer model

Supported OS:

Windows XP
Windows Vista
Windows 7
Windows 8
Windows 8.1
Windows 10

Installation procedure:

a) Serial interface
For a serial interface printer you may execute the standard
printer installation procedure or follow the automatic wizard procedure.
For standard printer installation the needed the files that are stored into: "..\CeTmpDrv" directory.

b) USB interface
Please follow the automatic wizard procedure.

This driver supports the model:
"CUSTOM VKP80III"

"CUSTOM VKP80III" can print on the following paper widths:
a) 80mm paper width 
b) 70mm paper width 
c) 60mm paper width 
d) 56mm paper width 


The "CUSTOM VKP80III" printer supports the following page formats:

"VKP80III 80mm"
"VKP80III 120mm"
"VKP80III 160mm"
"VKP80III 200mm"
"VKP80III 240mm"
"VKP80III 280mm"
"VKP80III 400mm"
"VKP80III Roll"
"VKP80III Roll Short"

[ the defalut installation page is "VKP80III Roll" ]

If the system driver properties section shows other pages not here specified, 
you must select only the above mentioned pages format.

Note about BlackMark Feature:
 we suggest to use "VKP80III Roll" or "VKP80III Roll Short" page format when You use Notch Alignmemnt.

Note about PRINT QUALITY and PRINT DENSITY:
if "Color Printing Mode" is set to "Grayscale 4 bit", the only "Print Quality" allowed value is "High speed", 
and the maximum "Print Density" allowed value is "0%".
If a different value is selected, a defalut setting will be used.
