TPTCML driver package for CUSTOM SPA printer.

Supported operative systems:

- Windows XP   		
- Windows Vista 	
- Windows 7 	
- Windows 8 


Installation procedure:
a) Serial interface
For a serial interface printer you may execute the standard
printer installation procedure or follow the automatic wizard procedure.
For standard printer installation the needed file are stored into: "..\CeTmpDrv" directory.
b) USB interface
Follow the automatic wizard procedure.


This driver supports:
Custom TPTCML 60mm (200dpi)

Page Format supported by printer are:

Custom TPTCML 60mm (200dpi):
TPTCML Roll 60 mm
TPTCML Roll+ 60 mm
TPTCML Roll++ 60 mm
TPTCML 60x65 mm
TPTCML 60x125 mm
TPTCML 60x185 mm
TPTCML 60x245 mm

If the system driver properties section shows these page formats and others not here
specified, you must select only the page formats mentioned above.

NOTE:
Please configure printer with "$1D $65 $07 nL nH" command to use page formats "TPTCML Roll+ 60 mm"
and "TPTCML Roll++ 60 mm" if your printer is a TPTCML 60mm Dispenser.
You can find more information about "$1D $65 $07 nL nH" command on printer manual.

LEGENDA:
Symbol		Function
$		it shows the hexadecimal value of the (ex. $40 corresponds at HEX 40).
{ }		it shows the ASCII character ASCII not performable
n, m, t, x, y	these are extra paramethers and/or optionals that can change in different cases
