;X23T-1_MHL.inf Ver. 1.0
;Monitor INF file for Fujitsu Display X23T-1_MHL
;Copyright 2012 Fujitsu Technology Solutions

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%FTS_Mfg%
CatalogFile=X23T-1_MHL.cat
DriverVer=08/16/2012,1.0.0.0

;-------------------------------------------------
[ControlFlags]
ExcludeFromSelect.nt=Monitor\FUS081D
ExcludeFromSelect.nt=Monitor\FUS081E
ExcludeFromSelect.nt=Monitor\FUS081F

[SourceDisksNames]
1=%DISK%,,,

[SourceDisksFiles]
X23T-1_MHL.icm=1

[DestinationDirs]
DefaultDestDir=12
FTSX23T1.CopyFiles=23

; Manufacturers
;-------------------------------------------------
[Manufacturer]
%FTS_Mfg%=FTS_Mfg,NTx86,NTAMD64

[FTS_Mfg] 
%X23T-1a%=FTSX23T1a.Install, Monitor\FUS081D
%X23T-1h1%=FTSX23T1h1.Install, Monitor\FUS081E
%X23T-1h2%=FTSX23T1h2.Install, Monitor\FUS081F

[FTS_Mfg.NTx86] 
%X23T-1a%=FTSX23T1a.Install, Monitor\FUS081D
%X23T-1h1%=FTSX23T1h1.Install, Monitor\FUS081E
%X23T-1h2%=FTSX23T1h2.Install, Monitor\FUS081F

[FTS_Mfg.NTAMD64] 
%X23T-1a%=FTSX23T1a.Install, Monitor\FUS081D
%X23T-1h1%=FTSX23T1h1.Install, Monitor\FUS081E
%X23T-1h2%=FTSX23T1h2.Install, Monitor\FUS081F

; Install Sections
;-------------------------------------------------

[FTSX23T1a.Install]
DELReg=DEL_CURRENT_REG    
AddReg=FTSX23T1a.AddReg, 1920, DPMS
CopyFiles=FTSX23T1.CopyFiles

[FTSX23T1h1.Install]
DELReg=DEL_CURRENT_REG    
AddReg=FTSX23T1h1.AddReg, 1920, DPMS
CopyFiles=FTSX23T1.CopyFiles

[FTSX23T1h2.Install]
DELReg=DEL_CURRENT_REG    
AddReg=FTSX23T1h2.AddReg, 1920, DPMS
CopyFiles=FTSX23T1.CopyFiles
					     
; AddReg & DELReg sections
;-------------------------------------------------

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1920]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

; AddReg sections
;---------------------------------------------------------- 

[FTSX23T1a.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,56.0-76.0,+,+"
HKR,,ICMProfile,0,"X23T-1_MHL.icm"

[FTSX23T1h1.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,56.0-76.0,+,+"
HKR,,ICMProfile,0,"X23T-1_MHL.icm"

[FTSX23T1h2.AddReg]
HKR,"MODES\1920,1080",Mode1,,"15.0-82.0,49.0-76.0,+,+"
HKR,,ICMProfile,0,"X23T-1_MHL.icm"

;---------------------------------------------------------- 

[FTSX23T1.CopyFiles]
X23T-1_MHL.icm

;---------------------------------------------------------- 

[FTSX23T1a.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[FTSX23T1h1.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[FTSX23T1h2.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"

DISK="Fujitsu Drivers, Manuals & Utilities Display"
FTS_Mfg="Fujitsu Technology Solutions"	

X23T-1a="Fujitsu X23T-1_MHL (Analog)"
X23T-1h1="Fujitsu X23T-1_MHL (HDMI1)"
X23T-1h2="Fujitsu X23T-1_MHL (HDMI2)"
