; n20wmgx2.inf
; Setup information file for NEC MultiSync 20WMGX2 Monitor
;
; Copyright 2005, NEC Display Solutions,Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=n20wmgx2.cat
DriverVer=09/27/2005,1.05.0927.2317

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC6693
ExcludeFromSelect.nt=Monitor\NEC6694

[DestinationDirs]
20WMGX2.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
n20wmgx2.icm=1

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%20WMGX2-A%=20WMGX2-A.Install, Monitor\NEC6693
%20WMGX2-D%=20WMGX2-D.Install, Monitor\NEC6694

[NECDS.ntamd64]
%20WMGX2-A%=20WMGX2-A.Install.ntamd64, Monitor\NEC6693
%20WMGX2-D%=20WMGX2-D.Install.ntamd64, Monitor\NEC6694

[20WMGX2-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=20WMGX2-A.AddReg, 1680, DPMS
CopyFiles=20WMGX2.CopyFiles

[20WMGX2-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=20WMGX2-D.AddReg, 1680, DPMS
CopyFiles=20WMGX2.CopyFiles

[20WMGX2-A.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=20WMGX2-A.AddReg, 1680, DPMS
CopyFiles=20WMGX2.CopyFiles

[20WMGX2-D.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=20WMGX2-D.AddReg, 1680, DPMS
CopyFiles=20WMGX2.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1680]
HKR,,MaxResolution,,"1680,1050"

[DPMS]
HKR,,DPMS,,1

[20WMGX2-A.AddReg]
HKR,"MODES\1680,1050",Mode1,,"31.0-81.0,56.0-60.0,+,+"
HKR,,ICMProfile,0,"n20wmgx2.icm"

[20WMGX2-D.AddReg]
HKR,"MODES\1680,1050",Mode1,,"31.0-81.0,56.0-60.0,+,+"
HKR,,ICMProfile,0,"n20wmgx2.icm"

[20WMGX2.CopyFiles]
n20wmgx2.icm

[Strings]
NECDS="NEC"
20WMGX2-A="NEC MultiSync 20WMGX2(Analog)"
20WMGX2-D="NEC MultiSync 20WMGX2(Digital)"
Disk1="NEC Monitor Installation Disk"