;L21T-1 LED.INF Ver. 1.0
;Monitor INF file for Fujitsu Display L21T-1 LED
;Copyright 2015 Fujitsu Technology Solutions

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%FTS_Mfg%
CatalogFile=L21T-1_LED.cat
DriverVer=06/01/2015,1.0.0.0

;-------------------------------------------------
[ControlFlags]
ExcludeFromSelect.nt=Monitor\FUS0875
ExcludeFromSelect.nt=Monitor\FUS0876

[SourceDisksNames]
1=%DISK%,,,

[SourceDisksFiles]
L21T-1_LED.icm=1

[DestinationDirs]
DefaultDestDir=11
L21T-1 LED_VGA.CopyFiles=23
L21T-1 LED_DVI.CopyFiles=23

; Manufacturers
;-------------------------------------------------
[Manufacturer]
%FTS_Mfg%=FTS_Mfg,NTx86,NTAMD64

 [FTS_Mfg] 
%L21T-1 LED_VGA%=L21T-1 LED_VGA.Install, Monitor\FUS0875
%L21T-1 LED_DVI%=L21T-1 LED_DVI.Install, Monitor\FUS0876

 [FTS_Mfg.NTx86] 
%L21T-1 LED_VGA%=L21T-1 LED_VGA.Install, Monitor\FUS0875
%L21T-1 LED_DVI%=L21T-1 LED_DVI.Install, Monitor\FUS0876

 [FTS_Mfg.NTAMD64] 
%L21T-1 LED_VGA%=L21T-1 LED_VGA.Install, Monitor\FUS0875
%L21T-1 LED_DVI%=L21T-1 LED_DVI.Install, Monitor\FUS0876

; Install Sections
;-------------------------------------------------

[L21T-1 LED_VGA.Install]
DELReg=DEL_CURRENT_REG    
AddReg=L21T-1 LED_VGA.AddReg, 1920, DPMS
CopyFiles=L21T-1 LED_VGA.CopyFiles

[L21T-1 LED_DVI.Install]
DELReg=DEL_CURRENT_REG    
AddReg=L21T-1 LED_DVI.AddReg, 1920, DPMS
CopyFiles=L21T-1 LED_DVI.CopyFiles
					     
; AddReg & DELReg sections
;-------------------------------------------------

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1920]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

; AddReg sections
;---------------------------------------------------------- 

[L21T-1 LED_VGA.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,50.0-75.0,+,+"
HKR,,ICMProfile,0,"L21T-1_LED.icm"

[L21T-1 LED_DVI.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,50.0-75.0,+,+"
HKR,,ICMProfile,0,"L21T-1_LED.icm"

;---------------------------------------------------------- 

[L21T-1 LED_VGA.CopyFiles]
L21T-1_LED.icm

[L21T-1 LED_DVI.CopyFiles]
L21T-1_LED.icm

;---------------------------------------------------------- 

[L21T-1 LED_VGA.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[L21T-1 LED_DVI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"

DISK="Fujitsu Drivers, Manuals & Utilities Display"
FTS_Mfg="Fujitsu Technology Solutions"	

L21T-1 LED_VGA="Fujitsu L21T-1 LED (VGA)" 
L21T-1 LED_DVI="Fujitsu L21T-1 LED (DVI)" 