; Copyright 2018 AOP International (Europe) GmbH
; This is a Setup information file for monitors with ICM file.


[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%AOP%
Catalogfile=27HC2R P.cat
DriverVer=02/01/2019,1.0.0.0

[ControlFlags]
ExcludeFromSelect.nt=Monitor\AOP06F6
ExcludeFromSelect.nt=Monitor\AOP06F6
ExcludeFromSelect.nt=Monitor\AOP06F6


[DestinationDirs]
DefaultDestDir=11
06F6_H1.CopyFiles=23
06F6_H2.CopyFiles=23
06F6_P.CopyFiles=23


[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
27HC2R P.ICM=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%AOP%=AOP,ntamd64

[AOP]
%06F6_H1%=06F6_H1.Install, Monitor\AOP06F6
%06F6_H2%=06F6_H2.Install, Monitor\AOP06F6
%06F6_P%=06F6_P.Install, Monitor\AOP06F6

[AOP.ntx86]
%06F6_H1%=06F6_H1.Install, Monitor\AOP06F6
%06F6_H2%=06F6_H2.Install, Monitor\AOP06F6
%06F6_P%=06F6_P.Install, Monitor\AOP06F6

[AOP.ntamd64]
%06F6_H1%=06F6_H1.Install, Monitor\AOP06F6
%06F6_H2%=06F6_H2.Install, Monitor\AOP06F6
%06F6_P%=06F6_P.Install, Monitor\AOP06F6


[06F6_H1.Install]
DelReg=DEL_CURRENT_REG
AddReg=06F6_H1.AddReg
Copyfiles=06F6_H1.CopyFiles

[06F6_H1.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install


[06F6_H2.Install]
DelReg=DEL_CURRENT_REG
AddReg=06F6_H2.AddReg
Copyfiles=06F6_H2.CopyFiles

[06F6_H2.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[06F6_P.Install]
DelReg=DEL_CURRENT_REG
AddReg=06F6_P.AddReg
Copyfiles=06F6_P.CopyFiles

[06F6_P.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install



[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[06F6_H1.AddReg]
HKR,"MODES\1920,1080",Mode1,,"15.0-180.0,48.0-120.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"27HC2R P.icm"

[06F6_H2.AddReg]
HKR,"MODES\1920,1080",Mode1,,"15.0-180.0,48.0-165.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"27HC2R P.icm"

[06F6_P.AddReg]
HKR,"MODES\1920,1080",Mode1,,"180.0-180.0,48.0-165.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"27HC2R P.icm"

[06F6_H1.CopyFiles]
27HC2R P.icm

[06F6_H2.CopyFiles]
27HC2R P.icm

[06F6_P.CopyFiles]
27HC2R P.icm

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

AOP="AOP International (Europe) GmbH"
DiskName="AOP Monitor Installation Disk"

06F6_H1="AOP 27HC2R P"
06F6_H2="AOP 27HC2R P"
06F6_P="AOP 27HC2R P"