;=======================================================
; P27T-7.INF Ver. 1.0 (for Windows 8) 06/26/2012
;
; Monitor INF file for Fujitsu Display P27T-T LED
;
; Copyright 2012 Fujitsu Technology Solutions GmbH
;=======================================================

[Version]
Signature   = "$Windows NT$"
Class       = Monitor
ClassGuid   = {4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider    = %FTS-Mfg%
CatalogFile = P27T-7.cat
DriverVer   = 06/26/2012, 1.0.0.0

[SourceDisksNames]
1 = %DiskName%

[SourceDisksFiles]
P27T-7.icm = 1

[DestinationDirs]
DefaultDestDir   = 12
P27T-7.Copyfiles = 23

[ControlFlags]
ExcludeFromSelect = Monitor\FUS0820
ExcludeFromSelect = Monitor\FUS0821
ExcludeFromSelect = Monitor\FUS0822
ExcludeFromSelect = Monitor\FUS0823

[Manufacturer]
%FTS-Mfg% = FTS-Mfg, NTx86, NTAMD64

[FTS-Mfg]
%P27T-7-a%  = P27T-7_a.Install, Monitor\FUS0820
%P27T-7-d%  = P27T-7_d.Install, Monitor\FUS0821
%P27T-7-h%  = P27T-7_h.Install, Monitor\FUS0822
%P27T-7-dp% = P27T-7_dp.Install, Monitor\FUS0823

[FTS-Mfg.NTx86]
%P27T-7-a%  = P27T-7_a.Install, Monitor\FUS0820
%P27T-7-d%  = P27T-7_d.Install, Monitor\FUS0821
%P27T-7-h%  = P27T-7_h.Install, Monitor\FUS0822
%P27T-7-dp% = P27T-7_dp.Install, Monitor\FUS0823

[FTS-Mfg.NTAMD64]
%P27T-7-a%  = P27T-7_a.Install, Monitor\FUS0820
%P27T-7-d%  = P27T-7_d.Install, Monitor\FUS0821
%P27T-7-h%  = P27T-7_h.Install, Monitor\FUS0822
%P27T-7-dp% = P27T-7_dp.Install, Monitor\FUS0823

[P27T-7_a.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P27T-7_a.AddReg, 1920x1200, DPMS
CopyFiles = P27T-7.CopyFiles

[P27T-7_d.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P27T-7_d.AddReg, 2560x1440, DPMS
CopyFiles = P27T-7.CopyFiles

[P27T-7_h.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P27T-7_h.AddReg, 1920x1080, DPMS
CopyFiles = P27T-7.CopyFiles

[P27T-7_dp.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P27T-7_d.AddReg, 2560x1440, DPMS
CopyFiles = P27T-7.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[P27T-7_a.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30.0-82.0,56.0-76.0,-,+"
HKR,,ICMProfile,0,"P27T-7.icm"

[P27T-7_d.AddReg]
HKR,"MODES\2560,1440",Mode1,,"30.0-100.0,56.0-76.0,+,-"
HKR,,ICMProfile,0,"P27T-7.icm"

[P27T-7_h.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-100.0,56.0-76.0,+,+"
HKR,,ICMProfile,0,"P27T-7.icm"

[1920x1080]
HKR,,MaxResolution,,"1920,1080"

[1920x1200]
HKR,,MaxResolution,,"1920,1200"

[2560x1440]
HKR,,MaxResolution,,"2560,1440"

[DPMS]
HKR,,DPMS,,1

[P27T-7.CopyFiles]
P27T-7.icm

[P27T-7.a.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P27T-7.d.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P27T-7.h.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P27T-7.dp.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"
FTS-Mfg         = "Fujitsu Technology Solutions"
DiskName        = "Fujitsu Monitor Installation Disk"

P27T-7-a        = "Fujitsu P27T-7 LED (Analog)"
P27T-7-d        = "Fujitsu P27T-7 LED (Digital)"
P27T-7-h        = "Fujitsu P27T-7 LED (HDMI)"
P27T-7-dp       = "Fujitsu P27T-7 LED (DP)"
