; as203wmi.inf
; Setup information file for NEC AS203WMi Monitor
;
; Copyright 2014, NEC Display Solutions, Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=as203wmi.cat
DriverVer=03/19/2014,1.14.0319.1546

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC2B38
ExcludeFromSelect.nt=Monitor\NEC2B39

[DestinationDirs]
AS203WMi.CopyFiles = 23
DefaultDestDir = 11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
as203wmi.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%AS203WMi-A%=AS203WMi-A.Install, Monitor\NEC2B38
%AS203WMi-D%=AS203WMi-D.Install, Monitor\NEC2B39

[NECDS.ntamd64]
%AS203WMi-A%=AS203WMi-A.Install.ntamd64, Monitor\NEC2B38
%AS203WMi-D%=AS203WMi-D.Install.ntamd64, Monitor\NEC2B39

[AS203WMi-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=AS203WMi-A.AddReg, 1600, DPMS
CopyFiles=AS203WMi.CopyFiles

[AS203WMi-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=AS203WMi-D.AddReg, 1600, DPMS
CopyFiles=AS203WMi.CopyFiles

[AS203WMi-A.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=AS203WMi-A.AddReg, 1600, DPMS
CopyFiles=AS203WMi.CopyFiles

[AS203WMi-D.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=AS203WMi-D.AddReg, 1600, DPMS
CopyFiles=AS203WMi.CopyFiles

[AS203WMi.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[AS203WMi.Install.ntamd64.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1600]
HKR,,MaxResolution,,"1600,900"

[DPMS]
HKR,,DPMS,,1

[AS203WMi-A.AddReg]
HKR,"MODES\1600,900",Mode1,,"31.0-83.0,55.0-76.0,+,+"
HKR,,ICMProfile,0,"as203wmi.icm"

[AS203WMi-D.AddReg]
HKR,"MODES\1600,900",Mode1,,"31.0-83.0,55.0-76.0,+,+"
HKR,,ICMProfile,0,"as203wmi.icm"

[AS203WMi.CopyFiles]
as203wmi.icm

[Strings]
NECDS="NEC"
AS203WMi-A="NEC AS203WMi(Analog)"
AS203WMi-D="NEC AS203WMi(Digital)"
Disk1="NEC Display Solutions Installation Disk"

SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

AS203WMi="NEC AS203WMi"
